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4: Hold     on       off

2: Drive    off       off

1: Drive    on       off

ALARM / RESET

Torque setting  (Nm)

< on   off >

3:

(0.7)     (1.5)

(1.0)    (2.5)
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1. CMR-01
Control Motor Rack 

Unit serial no. _________
Hardware revision _________ 

2. CMP-01
Control Motor Power 

Unit serial no. _________
Hardware revision _________ 

3. CMD-RM2 Control Motor Driver 

Unit serial no. _________
Hardware revision _________ 

DIP settings

actual

default


4-pole dip switch in the front
left
right 
left
right

1. Drive 1

(
(
(
(

Drive current 1

2. Drive 2 

(
(
(
(

Drive current 2

3.


(
(
(
(

Not used

4. Hold

(
(
(
(

Hold current

No limit adjustments on this unit.
4. CMI-01 Control Motor Interface 

Unit serial no. _________
Hardware revision _________ 
Software revision _________
DIP settings

actual

default


Function

off
on
off
on

Adjust screw pitch
SW2/1
(
(
(
(
Adjust screw pitch
SW2/2
(
(
(
(
CMD-RM1/CMD-RM2
SW2/3
(
(
(
(
Reverse direction (-RM2)
SW2/4
(
(
(
(
Speed adjustments

actual

default
Highspeed (H_sp)

-

100 %
Lowspeed (L_sp)

-

76 %

5. CONTACT
[image: image5.jpg]Valmet >



Sales, development, production and service:

Dametric AB

Jägerhorns Väg 19, SE 141 75 Kungens Kurva, Sweden

Phone:  +46-8 556 477 00
Telefax: +46-8 556 477 29

E-Mail: service@dametric.se
Website: www.dametric.se
[image: image1.png]



CMS-11-15 PAR EN.doc
Nov. 21, 2012
2(2)

