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AGS - Calibration
· Inform the operator that the refiner will be calibrated, meaning that no changes in the process must be done.

· Press Menu.
· Press Login, enter 1212, press OK, press Close.

· Press AGS Service.

· Press Auto Calibrate.

· Press Run.

· Wait until the calibration sequence is finished, takes about 20-40 seconds.

· Compare the current Gap to what the new Gap will be if accepted.
Press Accept if satisfied and the new calibration will be used, or…
…press No to decline the calibration and the old values are still valid.
· Press Close to exit the Auto Calibration form.
· Press Logout.
· Press Close to leave the AGS Service form.
· Press Close to leave the Menu form.
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