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1. UNITS

Unit
Description
Serial no. 
HW rev.
SW rev.
Refiner
Valmet RGP-?
R?
RMS-CD1
RMS Rack
?
2.0
CMD-RM1/2
Control Motor Driver
?
6.2
CMI-RM1
Control Motor Interface
?
6.1
4.2

MPM-RM1/2
Motor Power Monitor
?
3.0
1.1
VIM-RM1 
Vibration Monitor
?
8.1
POM-RM1 (c)
Position Monitor
?
9.0

POM-RM1 (f)
Position Monitor
?
9.0

TVD-RM1/3 (c)
Touchpoint Monitor
?
7.1
TVD-RM1/3 (f)
Touchpoint Monitor
?
7.1

DCU-RM2
Display Control Unit RMS-CD
?
8.0
7.09
DCA-RM1 (c)
Disc Clearance Amplifier
?
8.0
7.19
DCA-RM1 (f)
Disc Clearance Amplifier
?
8.0
7.19
DTM-RM1 (c)
Disc Temperature Monitor
?
6.1
DTM-RM1 (f)
Disc Temperature Monitor
?
6.1
HPM-RM1
Hydraulic Pressure Monitor
?
4.2

OTM-RM1 (1)
Oil Temperature Monitor
?
7.1

OTM-RM1 (2)
Oil Temperature Monitor
?
7.1

SSM-RM1
Safeset Monitor
?
3.0
2. DCU-RM2 
Menu
2, Activated units for the sum alarm check


Unit
actual
default

Disc temp. (CD)
DTMc
-
On+Alarm
Disc temp. (Flat)
DTMf
-
On+Alarm
Hydr. Pressure
HPM
-
Off
Motor Power
MPM
-
On+Alarm
Opt. Temp -1
OTM-1
-
On+Alarm
Opt. Temp -2
OTM-2
-
Off

Rotor Position (CD)
POMc
-
On+Alarm
Rotor Position (Flat)
POMf
-
On+Alarm
Touchpoint (CD)
TVDc
-
On+Alarm
Touchpoint (Flat)
TVDf 
-
On+Alarm
Vibration
VIM
-
On+Alarm
Note. The On+Alarm is applicable for DCU-RM2 units with 7.10 or higher software revision. Older version only use “on” or “off”.
Menu
3, Range settings
Unit
actual
 default


Main motor power
MPM
-
20.00 MW 

 
POMc Stroke
POM
-
50 mm 


POMf Stroke
POM
-
50 mm 

 
A-chamber Press
HPM-A
-
97.6 ton 

 
B-chamber Press
HPM-B
-
160.0 ton 


DCA CD-zone
DCAc
-
3.00 mm 


DCA Flat zone
DCAf
-
3.00 mm 
 
Reg. Hires.
-
-
0
Menu
4, DCA calibration settings



Unit
actual
default


TVDc Limit
TVD
-
50 %


TVDf Limit
TVD
-
50 %

Menu
5, CD-Zone Regulator settings
actual
default


Deadband

-
(0.05 mm 


Interval

- 
10 s 


Gain

-
100 %


Filter factor

- 
5 s 


Over alarm

- 
50 %


Speed limit (over alarm)
-
0.10 mm/min 


Under alarm

-
10 interval

Low A-pressure interlocking
-
Enabled 
Menu
6, Flat Zone Regulator settings
actual
default


Deadband

-
(0.05 mm 


Gain

-
100 %


Filter factor

- 
5 s 


Feed Forward together
- 
100 %


Feed Forward apart

- 
100 %


Gearbox turn-over play
- 
0.00 mm


Over alarm

- 
50 %


Speed limit (over alarm)
-
0.10 mm/min


Under alarm

-
10 interval 

Menu
7, Feed Guard settings
actual
default


Piston Length

-
3.00 mm 


Rotor Safe Distance

-
3.00 mm 


Timeout

- 
30 s 

Menu
11, Gap Guard settings
actual
default


Time

-
2 s 


Distance CD

-
25 % 


Distance Flat

-
25 % 


Gain CD

-
100 %


Gain Flat

-
100 %

Menu
9, CD segment holder type
actual
default


Segment holder type

 -
0.25
Menu
12, Display
actual
default

Display

- 
PDU-RM2 
3. CMD-RM2
CMD-DM2
actual
default
function
4-pole dip switch in the front
left
right 
left
right

1. Drive 1

(
(
(
(
Drive current 1

2. Drive 2 

(
(
(
(
Drive current 2

3.


(
(
(
(
Not used

4. Hold

(
(
(
(
Hold current

4. CMI-RM1
DIP settings
actual
default
Function

off
on
off
on

Adjust screw pitch
SW2/1
(
(
(
(
Adjust screw pitch
SW2/2
(
(
(
(
CMD-RM1/CMD-RM2
SW2/3
(
(
(
(
Reverse direction (-RM2)
SW2/4
(
(
(
(
Speed adjustments
actual
default
Highspeed (H_sp)

-
100 %
Lowspeed (L_sp)

-
76 %
5. MPM-RM1 / MPM-RM2
The nominal motor power is configured in the DCU-unit.

No dip settings on MPM-RM1. 

DIP settings MPM-RM2
actual
default



off
on
off
on

Use Limit 3 (Float)
SW4/1
(
(
(
(
Set to off if not used

Not used
SW4/2
(
(
(
(
Not used
SW4/3
(
(
(
(
Not used
SW4/4
(
(
(
(
Limit adjustments
actual
default (with 20.0 MW power setting)
Low
(L 1)

-
8.0 MW
LoLow (L 2)

-
2.0 MW
Floating (L 3 LEVEL)

-
4.0 MW
Floating (L 3 TIME)

-
3.0 s

Limit 3 (Floating) is only available for the MPM-RM2 unit.

6. VIM-RM1
Limit adjustments
actual
default
Limit 1 (L 1)

-
10 mm/s
Limit 2 (L 2)

-
8 mm/s
7. POM-RM1, CD-zone

Limit adjustments
actual
default
Limit 1 (L 1)

-
37.50 mm
Limit 2 (L 2)

-
25.00 mm
Limit 3 (L 3)

-
15.00 mm
8. POM-RM1, Flat zone

Limit adjustments
actual
default
Limit 1 (L 1)

-
25.00 mm
Limit 2 (L 2)

-
15.00 mm
Limit 3 (L 3)

-
4.00 mm
9. TVD-RM1 / TVD-RM3, CD-zone

DIP settings
actual
default
Transducer location attenuation
off
on
off
on

SW4 on the 9179 board
SW_/1
(
(
(
(
SW3 on the 9431 board
SW_/2
(
(
(
(


SW_/3
(
(
(
(


SW_/4
(
(
(
(
Low gain attenuation

off
on
off
on

SW3 on the 9179 board
SW_/1
(
(
(
(
SW4 on the 9431 board
SW_/2
(
(
(
(


SW_/3
(
(
(
(


SW_/4
(
(
(
(
Transducer type

off
on
off
on



SW5/1
(
(
(
(


SW5/2
(
(
(
(


SW5/3
(
(
(
(


SW5/4
(
(
(
(
Headset volume

off
on
off
on



SW2/1
(
(
(
(


SW2/2
(
(
(
(
Limit adjustments
actual
default
Limit 1 (L 1)

-
75 %


Limit 2 (L 2)

-
50 % 

10. TVD-RM1 / TVD-RM3, Flat zone

DIP settings
actual
default
Transducer location attenuation
off
on
off
on



SW3/1
(
(
(
(


SW3/2
(
(
(
(


SW3/3
(
(
(
(


SW3/4
(
(
(
(
Low gain attenuation

off
on
off
on



SW4/1
(
(
(
(


SW4/2
(
(
(
(


SW4/3
(
(
(
(


SW4/4
(
(
(
(
Transducer type

off
on
off
on



SW5/1
(
(
(
(


SW5/2
(
(
(
(


SW5/3
(
(
(
(


SW5/4
(
(
(
(
Headset volume

off
on
off
on



SW2/1
(
(
(
(


SW2/2
(
(
(
(
Limit adjustments
actual
default
Limit 1 (L 1)

-
75 %
Limit 2 (L 2)

-
50 %
11. DCA-RM1, CD-zone

DIP settings
actual
default



off
on
off
on

Main motor speed
SW6/1
(
(
(
(
Main motor speed
SW6/2
(
(
(
(
Decreased measure time
SW6/3
(
(
(
(
Decreased measure time
SW6/4
(
(
(
(
Increased measure time
SW7/1
(
(
(
(
Increased measure time
SW7/2
(
(
(
(
Off=TDC/On=AGS
SW7/3
(
(
(
(
Transducer check
SW7/4
(
(
(
(
Flat/conical zone
SW8/1
(
(
(
(
Enable push-buttons
SW8/2
(
(
(
(
Measure range
SW8/3
(
(
(
(
Response time
SW8/4
(
(
(
(
Not used
SW9/1-4
(
(
(
(
Limit adjustments
actual
default
Limit 1 + + (L1)

-
1.20 mm

Limit 2 +    (L2)

-
1.00 mm 

Limit 1 -     (L3)

-
0.50 mm

Limit 2 - -   (L4)

-
0.30 mm

12. DCA-RM1, Flat zone

DIP settings
actual
default



off
on
off
on

Main motor speed
SW6/1
(
(
(
(
Main motor speed
SW6/2
(
(
(
(
Decreased measure time
SW6/3
(
(
(
(
Decreased measure time
SW6/4
(
(
(
(
Increased measure time
SW7/1
(
(
(
(
Increased measure time
SW7/2
(
(
(
(
Off=TDC/On=AGS
SW7/3
(
(
(
(
Transducer check 
SW7/4
(
(
(
(
Flat/conical zone
SW8/1
(
(
(
(
Enable push-buttons
SW8/2
(
(
(
(
Measure range
SW8/3
(
(
(
(
Response time
SW8/4
(
(
(
(
Not used
SW9/1-4
(
(
(
(
Limit adjustments
actual
default
Limit 1 + + (L1)

-
1.60 mm

Limit 2 +    (L2)

-
1.40 mm 

Limit 1 -     (L3)

-
0.60 mm

Limit 2 - -   (L4)

-
0.40 mm
13. DTM-RM1, CD-zone
Limit adjustments
actual
default
Limit 1 (L1)

-
200 º
Limit 2 (L2)

-
170 º
Limit 3 (L3)

-
90 º

14. DTM-RM1,  Flat zone

Limit adjustments
actual
default
Limit 1 (L1)

-
200 º
Limit 2 (L2)

-
170 º
Limit 3 (L3)

-
90 º
15. HPM-RM1
Limit adjustments
actual
default 
A-Chamber pressure, Limit 1
-
3.5 ton (with 97.6 ton HPM-A setting)
A-Chamber pressure, Limit 2
-
32 ton
B-Chamber pressure, Limit 1
-
96 ton (with 160 ton HPM-B setting)
B-Chamber pressure, Limit 2
-
64 ton

16. OTM-RM1 / 1
DIP settings
actual
default (100(C)



off
on
off
on



SW2/1
(
(
(
(


SW2/2
(
(
(
(


SW2/3
(
(
(
(


SW2/4
(
(
(
(
All 4 must either be off or on: 100 (C - set all to off, 200 (C - set all to on.

Limit adjustments 
actual
default (with 100(C range)
Channel 1, Limit 1 (C1L1)

-
60 °C 
Channel 1, Limit 2 (C1L2)

-
50 °C 
Channel 2, Limit 1 (C2L1)

-
60 °C 
Channel 2, Limit 2 (C2L2)

-
50 °C 
17. OTM-RM1 / 2
DIP settings 
actual
default (100(C)



off
on
off
on



SW2/1
(
(
(
(


SW2/2
(
(
(
(


SW2/3
(
(
(
(


SW2/4
(
(
(
(
All 4 must either be off or on: 100 (C - set all to off, 200 (C - set all to on.

Limit adjustments 
actual
default (with 100(C range)
Channel 1, Limit 1 (C1L1)

-
60 °C 
Channel 1, Limit 2 (C1L2)

-
50 °C 
Channel 2, Limit 1 (C2L1)

-
60 °C 
Channel 2, Limit 2 (C2L2)

-
50 °C 

18. SSM-RM1, Option unit

DIP settings
actual
default



off
on
off
on

Rotation time
SW2/1
(
(
(
(
Reset

SW2/2
(
(
(
(
Measure dir. of rotation
SW2/3
(
(
(
(
Not used
SW2/4
(
(
(
(
Fault pulses (0-9)
SW3
-

4

19. CONTACT
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Sales, development, production and service:

Dametric AB

Jägerhorns Väg 19, 141 75 Kungens Kurva, Sweden

Phone:  +46-8 556 477 00
Telefax: +46-8 556 477 29

e-mail: service@dametric.se
Web site: www.dametric.se
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