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1. UNITS

Unit
Description
Serial no. 
HW rev.
SW rev.
Refiner
Valmet RGP-?
R?

RMS-RS1
RMS Rack
?
3.1
DCM-RM1
Disc Clearance Module
?
6.1
1.70
RPU-RM1/RM2
RMS Power Unit
?
1.0

RRU-RM1 (1)
RMS Relay Unit
?
2.0
RRU-RM1 (2)
RMS Relay Unit
?
2.0
POM-RM1
Position Monitor
?
9.0

TVD-RM1/3
Touchpoint Monitor
?
7.1
VIM-RM1 
Vibration Monitor
?
8.1
MPM-RM1/2
Motor Power Monitor
?
3.0
1.1

HPM-RM1
Hydraulic Pressure Monitor
?
4.2

OTM-RM1 (1)
Oil Temperature Monitor
?
7.1

OTM-RM1 (2)
Oil Temperature Monitor
?
7.1
DXM-DM1
Digital Extension Module
? 
2.0
1.04
2. DCM-RM1
Parameters
current
standard
adjustment range

Motor Speed
-
1500
480-3000 rpm

TDC Range
-
2.00
2.00 / 3.00 / 4.50 mm
DCA Filter
-
2
0.5 / 10 Hz

TVD Cal. Level
-
50
10 / 100 %

TDC Zero Par
-
0.50
0.10 / 1.50 mm

TDC Span Par
-
1.50
0.70 / 2.00 mm
POM Coarse Interlock
-
0.00
0.00 / 50.00 mm

MPM Power
-
5.0
0.1 / 50.0 MW
HPM A-Press
-
50.0
10.0 / 150.0 ton
HPM B-Press
-
50.0
10.0 / 150.0 ton
Gap/POM ratio
-
1.00
0.01-1.00 

CAN node no.
-
0
0 / 2

RMS System
-
TDC
TDC/AGS-SD/…

*FG Timeout
-
10
0/60

*FG Pist. len.
-
1.00
0.00/9.00

*FG Safe dist.
-
1.00
0.00/9.00

* = selectable if DXM is set to ”ON_CAN” under ’Units’ below.

DCM Limits
current
standard
adjustment range

TDC ++
-
1.20
0.20 / 3.00 mm

TDC +
-
1.10
0.20 / 3.00 mm

TDC SP
-
0.75
0.20 / 3.00 mm

TDC -
-
0.50
0.20 / 3.00 mm

TDC --
-
0.30
0.20 / 3.00 mm

DTM1 (high)
-
200
0 / 250 °C

DTM2 (low)
-
150
0 / 250 °C

Units

current
standard
adjustment range

DTM

-
ON
ON/OFF

POM

-
ON
ON/OFF

TVD

-
ON
ON1/ON2/OFF

VIM

-
OFF
ON1/ON2/OFF

OTM-1
-
OFF
ON1/ON2/OFF

OTM-2
-
OFF
ON1/ON2/OFF

MPM

-
OFF
ON1/ON2/OFF

HPM

-
OFF
ON1/ON2/OFF
DXM

-

OFF
OFF/ON_CAN

3. POM-RM1
Alarm limit settings
current
standard 
adjustment range
Limit 1 (L 1)
-

39.00 mm 
0 – 50 mm
Limit 2 (L 2)
-

30.00 mm
0 – 50 mm
Limit 3 (L 3)
-

28.00 mm
0 – 50 mm
4. TVD-RM1

DIP settings
current
standard
Damper kit for sensor placement
off
on
off
on



SW3/1
(
(
(
(


SW3/2
(
(
(
(


SW3/3
(
(
(
(


SW3/4
(
(
(
(
Damper kit for production
off
on
off
on



SW4/1
(
(
(
(


SW4/2
(
(
(
(


SW4/3
(
(
(
(


SW4/4
(
(
(
(
Headset volume

off
on
off
on



SW2/1
(
(
(
(


SW2/2
(
(
(
(
Alarm limit settings
current
standard 
adjustment range
Limit 1 (L 1)
-

75 %
0 – 100 %

Limit 2 (L 2)
-

50 % 
0 – 100 %

5. VIM-RM1

(Optional unit)

No DIP settings on this unit.
Alarm limit settings
current
standard 
adjustment range
Limit 1 (L 1)
-

10 mm/s
0 – 25 mm/s
Limit 2 (L 2)
-

8 mm/s
0 – 25 mm/s
6. MPM-RM1 / MPM-RM2
(Optional unit)

Nominal motor power is configured in the LDU unit. See the PRO-EX1 manual.
No DIP settings on MPM-RM1. 
DIP settings MPM-RM2
current
standard



off
on
off
on
Use setting 3 (floating) SW4/1
(
(
(
(
Set to off if not used.
Not used
SW4/2
(
(
(
(
Not used
SW4/3
(
(
(
(
Not used
SW4/4
(
(
(
(
Alarm limit settings
current
standard 
adjustment range
Low
(L 1)
-

5.0 MW
0.1 – 50 MW
Low-low (L 2)
-

1.0 MW
0.1 – 50 MW

Floating (L 3 LEVEL)
-

3.0 MW
0.1 – 50 MW
Floating (L 3 TIME)
-

3.0 s
0 – 10 s

Limit 3 (floating) exists only for the MPM-RM2.



7. HPM-RM1

(Optional unit)

Alarm limit settings
current
standard 
adjustment range
Channel 1, Limit 1 (A chamber)
-

3.0 ton
10 – 150 ton
Channel 1, Limit 2 (A chamber)
-

5.0 ton
10 – 150 ton
Channel 2, Limit 1 (B chamber)
-

50.0 ton
10 – 150 ton
Channel 2, Limit 2 (B chamber)
-

60.0 ton
10 – 150 ton
8. OTM-RM1 (1)
(Optional unit)

DIP settings
current
standard (100 (C)



off
on
off
on


SW1/1
(
(
(
(


SW1/2
(
(
(
(


SW1/3
(
(
(
(


SW1/4
(
(
(
(
All 4 must be in the off or on position: 
100 °C – set all to off, 200 °C - set all to on.
Alarm limit settings
current
standard (100 °C) adjustment range (100 °C)
Channel 1, Limit 1 (C1L1)
-

60 °C 
0 - 100 °C
Channel 1, Limit 2 (C1L2)
-

55 °C 
0 - 100 °C
Channel 2, Limit 1 (C1L1)
-

60 °C 
0 - 100 °C
Channel 2, Limit 2 (C1L2)
-

55 °C 
0 - 100 °C
9. OTM-RM1 (2)
(Optional unit)

DIP settings
current
standard (100 (C)



off
on
off
on


SW1/1
(
(
(
(


SW1/2
(
(
(
(


SW1/3
(
(
(
(


SW1/4
(
(
(
(
All 4 must be in the off or on position: 
100 °C – set all to off, 200 °C - set all to on.
Alarm limit settings
current
standard (100 °C) adjustment range (100 °C)
Channel 1, Limit 1 (C1L1)
-

60 °C 
0 - 100 °C
Channel 1, Limit 2 (C1L2)
-

55 °C 
0 - 100 °C
Channel 2, Limit 1 (C1L1)
-

60 °C 
0 - 100 °C
Channel 2, Limit 2 (C1L2)
-

55 °C 
0 - 100 °C
10. REVISIONS

Aug. 27, 2007
Updated for DCM-RM1 version 1.60 with higher measuring range.

Nov. 2, 2010
The third DTM limit is replaced by a fifth TDC limit (TDC-SP).

April 29, 2011
Added serial numbers and revision for the units.

Aug. 1, 2014
Valmet.

11. CONTACT
Development, production and maintenance:
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Dametric AB

Jägerhorns väg 19, SE-141 75 Kungens Kurva, Sweden

Phone: +46 (0)8-556 477 00
Fax: +46 (0)8-556 477 29

E-mail: service@dametric.se
Website: www.dametric.se
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