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1. UNITS

Unit
Description
Serial no. 
HW rev.
SW rev.
Refiner
Valmet RGP-?
R?

RMS-SD1
RMS Rack
?
2.0
CMD-RM2
Control Motor Driver
?
6.2
CMI-RM1
Control Motor Interface
?
6.1
4.2

MPM-RM2
Motor Power Monitor
?
3.0
1.1
VIM-RM1 
Vibration Monitor
?
8.1
POM-RM1
Position Monitor
?
9.0

TVD-RM1
Touchpoint Monitor
?
7.1
DCU-RM1
Display Control Unit RMS-SD
?
8.0
7.06
DCA-RM1
Disc Clearance Amplifier
?
8.0
7.18
DTM-RM1
Disc Temperature Monitor
?
6.1
HPM-RM1
Hydraulic Pressure Monitor
?
4.2

OTM-RM1 (1)
Oil Temperature Monitor
?
7.1

OTM-RM1 (2)
Oil Temperature Monitor
?
7.1

SSM-RM1
Safeset Monitor
?
3.0
2. DCU-RM1
Activated units for the sum alarm check
Menu

Unit
actual
default

2
Disc temp.
DTM
- 
on 


Hydr. Pressure
HPM
- 
off 


Motor Power
MPM
- 
on 


Opt. Temp -1
OTM-1
- 
off 


Opt. Temp -2
OTM-2
- 
off 


Opt. Temp -3
OTM-3
- 
off 


Opt. Temp -4
OTM-4
- 
off 


Opt. Temp –5
OTM-5
- 
off 


Opt. Temp –6
OTM-6
- 
off 


Rotor Position
POM
- 
on 


Touchpoint
TVD
- 
on 


Vibration
VIM
- 
on 


Vibration
VIMf
- 
off 

Range setting

Menu

Unit
actual
default

3
Motor Power
MPM
-
5.00 MW

 
Pom Stroke
POM
-
50 mm

 
A-chamber Press.
HPM-A
-
50.0 ton

 
B-chamber Press.
HPM-B
-
50.0 ton


DCA Range
DCA
-
2.00 mm

RMS System
RMS
- 
SD 

DCA calibration setting

Menu

Unit
actual
default

4
TVD Limit
TVD
-
50 %


POM Ratio
POM
-
1

Regulator setting 


Menu


actual
default

5
Deadband

-
0.05 mm 


Interval

- 
10 s 


Gain

-
100 %


Filter factor

- 
5 s 


Over alarm

- 
50 %


Speed limit (over alarm)
-
1.00 mm/min 


Under alarm

-
10 Interval

Low A-Pressure

-
Enabled

Gap Guard settings

Menu


actual
default

11
Time

-
2 s 


Deviate

-
25 % 


Gain

-
100 %

Feed Guard settings

Menu


actual
default

6
Piston Length

-
1.00 mm 


Safe Distance

-
1.00 mm 


Timeout

- 
10 s 

Display

Menu


actual
default
12
PDU

- 
on 

OP-Panel

-
-

PanelPC

-
-
3. CMD-RM2
DIP settings
actual
default
function
4-pole dip switch in the front
left
right 
left
right

1. Drive 1

(
(
(
(
Drive current 1

2. Drive 2

(
(
(
(
Drive current 2

3.


(
(
(
(
Not used

4. Hold

(
(
(
(
Hold current

4. CMI-RM1
Dip settings
actual
default
Function

off
on
off
on

Adjust screw pitch
SW2/1
(
(
(
(
Adjust screw pitch
SW2/2
(
(
(
(
CMD-RM1/2
SW2/3
(
(
(
(
Reverse direction (-RM2)
SW2/4
(
(
(
(
Speed adjustments
actual
default
High speed (H_sp)

-
100 %
Low speed (L_sp)

-
100 %
5. MPM-RM1 / MPM-RM2
The nominal motor power is configured in the DCU-unit.

No dip settings on MPM-RM1. 

Dip settings MPM-RM2
actual
default



off
on
off
on

Use Limit 3 (Float)
SW4/1
(
(
(
(
Set to off if not used

Not used
SW4/2
(
(
(
(
Not used
SW4/3
(
(
(
(
Not used
SW4/4
(
(
(
(
Limit adjustments
actual
default
Low
(L 1)

-
40 % of P
Lolow (L 2)

-
20 % of P
Floating (L 3 LEVEL)

-
20 % of P
Floating (L 3 TIME)

-
3.0 s

Limit 3 (Floating) is only available for the MPM-RM2 unit.
P is the programmed motor power.
6. VIM-RM1
Limit adjustments
actual
default
Limit 1 (L 1)

-
10 mm/s
Limit 2 (L 2)

-
8 mm/s
7. POM-RM1
Limit adjustments
actual
default
Limit 1 (L 1)

-
39.00 mm

Limit 2 (L 2)

-
30.00 mm

Limit 3 (L 3)

-
28.00 mm
8. TVD-RM1
Dip settings
actual
default
Transducer location attenuation
off
on
off
on



SW3/1
(
(
(
(


SW3/2
(
(
(
(


SW3/3
(
(
(
(


SW3/4
(
(
(
(
Low gain attenuation

off
on
off
on



SW4/1
(
(
(
(


SW4/2
(
(
(
(


SW4/3
(
(
(
(


SW4/4
(
(
(
(
Headset volume

off
on
off
on



SW2/1
(
(
(
(


SW2/2
(
(
(
(
Limit adjustments
actual
default
Limit 1 (L 1)

-
75 %
Limit 2 (L 2)

-
50 % 
9. DCA-RM1
Dip settings
actual
default



off
on
off
on

Main motor speed
SW6/1
(
(
(
(
Main motor speed
SW6/2
(
(
(
(
Decreased measure time
SW6/3
(
(
(
(
Decreased measure time
SW6/4
(
(
(
(
Increased measure time
SW7/1
(
(
(
(
Increased measure time
SW7/2
(
(
(
(
Ags Sensor
SW7/3
(
(
(
(
Transducer check
SW7/4
(
(
(
(
Flat/conical zone
SW8/1
(
(
(
(
Enable push-buttons
SW8/2
(
(
(
(
Measure Range
SW8/3
(
(
(
(
Response time
SW8/4
(
(
(
(
Not used
SW9/1-4
(
(
(
(
Limit adjustments
actual
default
Limit 1 + + (L1)

-
1,20 mm

Limit 2 +    (L2)

-
0,90 mm

Limit 1 -     (L3)

-
0,70 mm

Limit 2 - -   (L4)

-
0,20 mm
10. DTM-RM1
No dip settings on this unit.

Limit adjustments
actual
default
Limit 1 (L1)

-
200 º
Limit 2 (L2)

-
170 º
Limit 3 (L3)

-
90 º
11. HPM-RM1
Limit adjustments
actual
default (with 50 ton HPM-range)
A-chamber pressure, Limit 1

-
3.3 ton
A- chamber pressure, Limit 2
-
10 ton
B- chamber pressure, Limit 1
-
20 ton
B- chamber pressure, Limit 2
-
10 ton
12. OTM-RM1 / 1
Dip settings
actual
default (100(C)



off
on
off
on



SW2/1
(
(
(
(


SW2/2
(
(
(
(


SW2/3
(
(
(
(


SW2/4
(
(
(
(
All 4 must either be off or on: 100 ºC - set all to off, 200 ºC - set all to on.

Limit adjustments 
actual
default (with 100(C range)
Channel 1, Limit 1 (C1L1)

-
60 °C 
Channel 1, Limit 2 (C1L2)

-
55 °C 
Channel 2, Limit 1 (C2L1)

-
60 °C 
Channel 2, Limit 2 (C2L2)

-
55 °C 
13. OTM-RM1 / 2
Dip settings 
actual
default (100(C)



off
on
off
on



SW2/1
(
(
(
(


SW2/2
(
(
(
(


SW2/3
(
(
(
(


SW2/4
(
(
(
(
All 4 must either be off or on: 100 ºC - set all to off, 200 ºC - set all to on.

Limit adjustments 
actual
default (with 100(C range)
Channel 1, Limit 1 (C1L1)

-
60 °C 
Channel 1, Limit 2 (C1L2)

-
55 °C 
Channel 2, Limit 1 (C2L1)

-
60 °C 
Channel 2, Limit 2 (C2L2)

-
55 °C 
14. OTM-RM1 / 3
Dip settings 
actual
default (100(C)



off
on
off
on



SW2/1
(
(
(
(


SW2/2
(
(
(
(


SW2/3
(
(
(
(


SW2/4
(
(
(
(
All 4 must either be off or on: 100 ºC - set all to off, 200 ºC - set all to on.

Limit adjustments 
actual
default (with 100(C range)
Channel 1, Limit 1 (C1L1)

-
60 °C 
Channel 1, Limit 2 (C1L2)

-
55 °C 
Channel 2, Limit 1 (C2L1)

-
60 °C 
Channel 2, Limit 2 (C2L2)

-
55 °C

15. OTM-RM1 / 4
Dip settings 
actual
default (100(C)



off
on
off
on



SW2/1
(
(
(
(


SW2/2
(
(
(
(


SW2/3
(
(
(
(


SW2/4
(
(
(
(
All 4 must either be off or on: 100 ºC - set all to off, 200 ºC - set all to on.

Limit adjustments 
actual
default (with 100(C range)
Channel 1, Limit 1 (C1L1)

-
60 °C 
Channel 1, Limit 2 (C1L2)

-
55 °C 
Channel 2, Limit 1 (C2L1)

-
60 °C 
Channel 2, Limit 2 (C2L2)

-
55 °C

16. OTM-RM1 / 5
Dip settings 
actual
default (100(C)



off
on
off
on



SW2/1
(
(
(
(


SW2/2
(
(
(
(


SW2/3
(
(
(
(


SW2/4
(
(
(
(
All 4 must either be off or on: 100 ºC - set all to off, 200 ºC - set all to on.

Limit adjustments 
actual
default (with 100(C range)
Channel 1, Limit 1 (C1L1)

-
60 °C 
Channel 1, Limit 2 (C1L2)

-
55 °C 
Channel 2, Limit 1 (C2L1)

-
60 °C 
Channel 2, Limit 2 (C2L2)

-
55 °C
17. OTM-RM1 / 6
Dip settings 
actual
default (100(C)



off
on
off
on



SW2/1
(
(
(
(


SW2/2
(
(
(
(


SW2/3
(
(
(
(


SW2/4
(
(
(
(
All 4 must either be off or on: 100 ºC - set all to off, 200 ºC - set all to on.

Limit adjustments 
actual
default (with 100(C range)
Channel 1, Limit 1 (C1L1)

-
60 °C 


Channel 1, Limit 2 (C1L2)

-
55 °C 


Channel 2, Limit 1 (C2L1)

-
60 °C 


Channel 2, Limit 2 (C2L2)

-
55 °C

18. SSM-RM1
Dip settings 
actual
default





off
on
off
on

Rotation time
SW2/1
(
(
(
(


Reset

SW2/2
(
(
(
(
Measure dir. of rotation
SW2/3
(
(
(
(
Not used
SW2/4
(
(
(
(
Fault pulses (0-9)
SW3
-

4

19. CONTACT
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Sales, development, production and service:

Dametric AB

Jägerhorns Väg 19, 141 75 Kungens Kurva, Sweden

Phone:  +46-8 556 477 00
Telefax: +46-8 556 477 29

E-mail: service@dametric.se
Web site: www.dametric.se
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